- Led connect power 🡪 set 0 will glow( light )

Uart – max232cpe

Led7 seg – url2803apg

Hy – 5461bs

Eeprom – altem 24c08

timer -

led matrix

bright H

rtc-sd1307

=================================================================================

0.kit

PROTO-063-BLE

1.chip

Psoc 4 – cy8c4245axi -473 PSoC 4

Psoc 4 – cy8c4245axi -483 PSoC 4

1.io-keyword-search-function

pin

digital output

digital input

resis – resistor

led

Vcc - power

switch

Vss – ground

interrupt

10.Command API

IO

led\_blue\_Write(1);

led\_blue\_Read();

flip flop???